- ADT cos hai thành phần của mô hình đó là Data struture và application program

- IPv4 có 32bit

-  components of a DBMS : Data Definition Language (DDL), Data Manipulation Language (DML), and Data Control Language (DCL).

-  unit is responsible for converting the data received from the user into a computer understandable format / input unit

- The only language which the computer understands is Binary Language

- The smallest unit of data in computer is Bit

- One nibble is equivalent to how many bits / 4

- describes the correct format of an input instruction / IN 82

-  The input machine which originated in the United States around 1880s is a / Keyboard

- What does the COMPUTER stand for? / Commonly Operated Machines Used in Technical and Educational Research

- Which of the following is not a function of the Input Unit? /  It makes the data into user understandable format

-  The process of producing useful information for the user is called / Outputting

- The output unit converts the data entered by the user into computer understandable form / False ( The Input Unit )

- VDU stands for / Visual Display Unit

- What does SVGA stand for / Super Video Graphics Array

-  The devices that used to give single or multiple colored images and drawings are / Plotters

-  A special request originated from some device to the CPU to acquire some of its time is called / Interrupt

- Line Printers that print one line at a time are / Drum Printers

- A \_\_\_ monitor looks like a television and are normally used with non-portable computer systems / CRT

- Which of the following is not a function of the Output Unit / It supplies the data and instructions to the computer for further processing

- PCI stands for  / Peripheral Component Interconnect

-  Components that provide internal storage to the CPU are / Registers

- Saving data and instructions to make them readily available is the job of / Storage Unit

- The two basic types of memory in a computer are / Primary and Secondary

-  Which of the following is used to hold running program instructions? / Primary Storage

- Which of the following is non-volatile storage? / Secondary

- Which of the following is used in main memory? / DRAM

- Which of the following are types of ROMs? / PROM & EPROM

- RAID stands for / Redundant array of independent disks

-  A non-erasable disk that stores digitized audio information is / CD