Name:

Class:

ID:

Given truth table as following:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A | B | C | D | F |
| 0 | 0 | 0 | 0 | 1 |
| 0 | 0 | 0 | 1 | 1 |
| 0 | 0 | 1 | 0 | 0 |
| 0 | 0 | 1 | 1 | 0 |
| 0 | 1 | 0 | 0 | 0 |
| 0 | 1 | 0 | 1 | 1 |
| 0 | 1 | 1 | 0 | 1 |
| 0 | 1 | 1 | 1 | 1 |
| 1 | 0 | 0 | 0 | 1 |
| 1 | 0 | 0 | 1 | 0 |
| 1 | 0 | 1 | 0 | 0 |
| 1 | 0 | 1 | 1 | 0 |
| 1 | 1 | 0 | 0 | 1 |
| 1 | 1 | 0 | 1 | 1 |
| 1 | 1 | 1 | 0 | 0 |
| 1 | 1 | 1 | 1 | 0 |

1. Define Boolean expression of F. (F is the function of A,B,C,D)
2. Using Boolean algebra, provide the simplified expression.
3. Using Karnaugh map, provide the simplified expression.
4. Design the intergrated circuit following the simplified expression of c.